# Proportional and Additive error model fitted to additive noise only synthetic data.

[Generated automatically as a Fitting summary]

## Inputs

### Description

Name: | ao_gen_pa_fit
Title: | Proportional and Additive error model fitted to additive noise only synthetic data.
Author: | Wright Dose Ltd
Abstract: |

One compartment model with a depot leading to a central compartment.
This model contains both proportional and additive error. The synthetic input data contains only additive noise and no proportional error.

Keywords: | one compartment model; dep_one_cmp_cl; proportional and additive error
Input Script: | `ao_gen_pa_fit.pyml`
Input Data: | `synthetic_data.csv`
Diagram: |

### Initial fixed effect estimates

    f[PNOISE_STD] = 0.5000
    f[ANOISE_STD] = 0.2500

## Outputs

### Final objective value

    -514.1872

which required 1.19 iterations and took 2.64 seconds

### Final fitted fixed effects

    f[PNOISE_STD] = 0.0010
    f[ANOISE_STD] = 0.0464

### Fitted parameter .csv files

Fixed Effects: | `fx_params.csv (fit)`
Random Effects: | `rx_params.csv (fit)`
Model params: | `mx_params.csv (fit)`
State values: | `sx_params.csv (fit)`
Predictions: | `px_params.csv (fit)`

## Plots

### Dense sim plots

Alternatively see All dense_sim graph plots

## Comparison

### Compare Main f[X]

### Compare Noise f[X]

Variable Name | Starting Value | Fitted Value | Prop Change | Abs Change
--- | --- | --- | --- | ---
f[PNOISE_STD] | 0.5000 | 0.0010 | 0.9980 | 0.4990
f[ANOISE_STD] | 0.2500 | 0.0464 | 0.8145 | 0.2036

### Compare Variance f[X]